Customer Loyalty

How It Works

A consumer with a TI-RFid tag in their purse, pocket, or wallet can be detected by reader systems at doorways. Readout antennas can also be in counters, walls, and in floors. The tag is powered by radio frequency signals issued from the reader. As the consumer passes by a reader system, the tag transmits its unique ID code to the reader. The reader then communicates this activation to a central database.